CARITO SMALL GRID POWER FRAME — HF212 EXAMPLE v1.0
==============================================

Document: SG-PF-HF212.txt
Status: Reference Example / Baseline-Oriented
Applies To: Small Grid (SG) Power Frame designs

--------------------------------------------------
1. IDENTIFICATION
--------------------------------------------------
Power Frame Name:
SG HF212 Baseline Power Frame

Power Frame Serial Identifier:
CAR-SG-PF-HF212-A-STD-R1

Grid:
SG (Small Grid)

Compatibility Class:
A (Baseline Compliant)

Revision:
R1

--------------------------------------------------
2. DESIGN SUMMARY
--------------------------------------------------
Intended Power System:
Single-cylinder commercial small engine (212cc class, HF-style)

Primary Use Case:
Baseline Small Grid internal combustion configuration

Baseline Eligible:
Yes

--------------------------------------------------
3. MMF INTERFACE
--------------------------------------------------
MMF Cage Type Compatibility:
TYPE-S, TYPE-R

Attachment Method:
Bolted with optional clamp assist

Removal Method:
Unbolt Power Frame from MMF hardpoint rails and lift as a unit

--------------------------------------------------
4. SLED DETAILS
--------------------------------------------------
Sled Type:
Engine sled

Engine Supported:
212cc class horizontal-shaft small engine

Isolation Method:
Rubber isolation mounts between engine and sled

--------------------------------------------------
5. CMZ CONFIGURATION
--------------------------------------------------
Conversion Type:
Chain reduction

Guarding Method:
Full chain guard with removable inspection cover

Adjustment Method:
Slotted sled mounts with lock bolts

--------------------------------------------------
6. ELECTRICAL (IF APPLICABLE)
--------------------------------------------------
Electrical Components Included:
Charging coil (optional), basic regulator

Voltage Levels:
12V accessory output

Routing Method:
Frame-mounted loom clips, no SPV intrusion

--------------------------------------------------
7. SPV COMPLIANCE
--------------------------------------------------
Fits Entirely Within SPV:
Yes

Service Access Zones Preserved:
Yes

--------------------------------------------------
8. MAINTENANCE AND SERVICE
--------------------------------------------------
Service Access Notes:
Top and side access to engine, chain, and carburetor

Tool Requirements:
Standard hand tools only

Expected Maintenance Intervals:
Per engine manufacturer recommendations

--------------------------------------------------
9. COMPATIBILITY IMPACT
--------------------------------------------------
Future Motor Compatibility Notes:
Power Frame removable without cutting; MMF cage unchanged

Upgrade or Replacement Path:
Replace Power Frame with alternative SG Power Frame

--------------------------------------------------
10. SAFETY AND COMPLIANCE
--------------------------------------------------
Guarding Compliance:
Chain fully guarded

Heat Management Notes:
Heat shield between exhaust and MMF cage

Noise and Vibration Notes:
Isolation mounts reduce vibration transfer

--------------------------------------------------
11. DECLARATIONS
--------------------------------------------------
This Power Frame:
[X] Does not modify MMF geometry
[X] Preserves declared compatibility class
[X] Accurately represents its configuration

Designer / Shop Name:
Reference Design

Date:
2026-01

Signature:
Platform Reference

--------------------------------------------------
END OF SG-PF-HF212 EXAMPLE
--------------------------------------------------
